C:\Users\alice\Desktop\2016 website\astekglobe logo.bmp [www.astekglobe.com](http://www.astekglobe.com)

ATA065 SERIES 60W DOE VI Adapter



Features

\*Universal AC Input Range

\*Protections: Short Circuit/Overload/ Overvoltage

\*DOE VI/ErP

\*Plastic case

\*1 year warranty

Application: IT/Industrial, Telecommunication, Network System, DVR(Digital Video Recorder) etc.

**Input**

Voltage: 90~264VAC

Frequency: 50~60Hz

Input current: 2ARMS @115VAC, 1ARMS@230VAC

Efficiency Level VI

**Output**

**Part No Rated O/P Ripple & Noise(mVp-p)**

**ATA065-S12-z 12V/5A 200**

**ATA065-S15-z 15V/4A 200**

**ATA065-S19-z 19V/3.42A 200**


**ATA065-S24-z 24V/2.7A 240**

**ATA065-S48-z 48V/1.35A 480**

**ATA065-S56-z 56V/1.16A 560**

**z: 14=C14, 06=C6, 08=C8**

**Mechanical Drawing** C14/C8/C6 inlet, Size: 123.12\*54.22\*35mm

****

Load Regulation: +/-5% Max.

Line Regulation: +/- 0.5% Max.

Over Load Protection/Short Circuit Protection: Hiccup/Auto Recovery

Over Voltage Protection: Latch Off

Operating Temperature: 0~40degree C

Storage Temperature: -40~85degree C

Storage Humidity: 5~95% RH

Safety approvals: DOE VI, UL, cUL,TUV-GS, CB, BSMI

EMC: CE, VCCI, LVD