 [www.astekglobe.com](http://www.astekglobe.com)

ATA090 SERIES 90W DOE VI Adapter



Features

\*Universal AC Input Range

\*Protections: Short Circuit/Overload/ Overvoltage

\*Efficiency: Level VI and V (optional)

\*DOE VI/ErP

\*Application: IT/Industrial, Telecommunication, Network System, DVR(Digital Video Recorder) etc.

**Input**

Voltage: 90~264VAC

Frequency: 50~60Hz

Efficiency Level VI

**Output**

**Part No Rated O/P**

**ATA090-S12-z 12V/7.5A**

**ATA090-S15-z 15V/6A**

**ATA090-S19-z 19V/4.74A**

**ATA090-S24-z 24V/3.75A**

**ATA090-S30-z 30V/3A**

**ATA090-S48-z 48V/1.875A**

**ATA090-S56-z 56V/1.607A**

**z: 14=C14, 06=C6, 08=C8**

**Mechanical Drawing** C14/C8/C6 inlet, Size: 148\*59\*32mm

****

Load Regulation: +/-5% Max.

Operating Temperature: 0~40degree C

Over Load Protection/Short Circuit Protection: Hiccup/Auto Recovery

Over Voltage Protection: Latch Off

Storage Temperature: -40~85degree C

Storage Humidity: 5~95% RH

Safety approvals: DOE VI, UL, cUL,TUV-GS, CB, BSMI

EMC: CE, VCCI, LVD