 **www.astekglobe.com**

APA065-24R SERIES 65W 15-24V Adjustable Output Voltage Adapter

Features

\*Universal AC Input Range

\*15-24V Adjustable Output Voltage Range

\*Protections: Short Circuit/Overload/ Overvoltage

\*Meet LVD

\*100% Hi-Pot & ATE Chroma test, 100% Burn-in test High Ambient Temp(45°C)

**Input**

Voltage: 90~264VAC

Frequency: 50~60Hz

Input current: 1.5A max.

Inrush current: 80A max

Efficiency Level V

**Output**

**Part No O/P Voltage O/P Current(max.) watt Max**

**APA065-S24R-z 15-24V(adjustable) 4.33A 65W**

**z: I=Interchangeable, 14=C14, 06=C6, 08=C8**

**AC plug: U=US, E=EU, A=Australia/New Zealand, B=British, K=Korean**

Load Regulation: 5% Max.

Line Regulation: 1% Max.

Operating Temperature: 0~40degree C

Storage Temperature: -20~85degree C

Over Voltage Protection/Short Circuit Protection: Auto Recovery

Ripple & Noise: 1%

Storage Humidity: 5~95% RH

Mechanical Type: Interchangeable US/EU/UK/AU/KR plug Cord-in Cord-out=C14/C6/C8 Inlet, US 2pin/3pin plug, EU/AS 2pin/3pin Plug, Desktop C14/C6/C8 inlet

Safety approvals: DOE V, UL, cUL,TUV-GS, CB
EMC: CE, VCCI, LVD
**Mechanical Drawing**

 Desktop Interchangeable Plug

  