 [www.astekglobe.com](http://www.astekglobe.com)

APA068 SERIES 65W Slim Adapter

Features

\*Universal AC Input Range

\*Meets EN55022 Class B and CISPR/FCC Class B

\*Protections: Short Circuit/Overload/ Overvoltage

\*Efficiency: Level V

\*Pass LPS/LVD

\*100% Hi-Pot & ATE Chroma test, 100% Burn-in test High Ambient Temp(45°C)

**Input**

Voltage: 90~264VAC

Frequency: 50~60Hz

Input current: 1.8A max.

Inrush current: 100A max

**Output**

Over Voltage Protection/Short Circuit Protection: Auto Recovery

Ripple & Noise: 1%

**Part No O/P Voltage O/P Current(max.) watt Max**

**APA068-S18-08 15~24V 3.42A 65W**

Load Regulation: 5% Max.

Line Regulation: 1% Max.

Efficiency Level V

Operating Temperature: 0~40degree C

Storage Temperature: -20~85degree C

Storage Humidity: 5~95% RH

Mechanical Type: Desktop C8 Inlet

Safety approvals: UL,cUL, CB,CE

EMC: CE, VCCI, LVD,FCC

Mechanical Drawing

Size: 110\*58\*18(mm)

 