 **www.astekglobe.com**

ATA050 SERIES 50W DOE VI Adapter



Features

\*Universal AC Input Range

\*Protections: Short Circuit/Overload/ Overvoltage

\*Efficiency: Level VI and V (optional)

\*DOE VI/ErP/ UL/cUL/TUV-GS/CB/BSMI/PSE/ CE/VCCI/LVD approved.

\*1 year warranty

**Input**

Voltage: 90~264VAC

Frequency: 50~60Hz

Input current: 1.2ARMS @115VAC

Efficiency Level VI

**Output**

**Part No Rated O/P Ripple & Noise(mVp-p)**

**ATA050-S12-z 12V/4.17A 240**

**ATA050-S15-z 15V/3.34A 240**

**ATA050-S19-z 19V/2.64A 240**

**ATA050-S24-z 24V/2.09A 240**

**ATA050-S48-z 48V/1.05A 480**

**ATA050-S56-z 56V/0.9A 560**

**z: 14=C14, 08=C8**

**Mechanical Drawing** C14/C8 inlet, Size: 117.6\*50.2\*31.6mm

****

Load Regulation: +/-5% Max.

Line Regulation: +/- 1% Max.

Over Load Protection/Short Circuit Protection: Hiccup/Auto Recovery

Over Voltage Protection: Latch Off

Operating Temperature: 0~40degree C

Storage Temperature: -40~85degree C

Storage Humidity: 5~95% RH

Safety approvals: DOE VI, UL, cUL,TUV-GS, CB, BSMI,PSE

EMC: CE, VCCI, LVD