 [www.astekglobe.com](http://www.astekglobe.com)

**APP015 15W Single Output Open Frame**

**Feature**

\*Over Voltage Protection, Over Current Protection, Short Circuit Protection

\*100% Burn in test at 40C

\*Low Ripple Noise

\*MTBF Above 50000 HRS at 25C

**Input**

Input Voltage: 90~264VAC
Input Current (Max): 0.4A

**Output**Output Voltage: 5V~48V
Output Power (Max): 15W
Ripple Noise: 1%
Efficiency: >=72%

**General Specifiction**Operating Temperature: 0~40 degree C
Storage Temperature: -20~85 degree C
Over Voltage Protection:Auto Recovery
Short Circuit Protecton: Auto Recovery
Meet CE, FCC
Dimension: 53.5\*37.5\*23mm

