 [www.astekglobe.com](http://www.astekglobe.com)

**APP020 20W Single Output Voltage Open Frame**

**Feature**

\*Over Voltage Protection, Over Current Protection, Short Circuit Protection

\*100% Burn in test at 40°C

\*Low Ripple Noise

\*MTBF Above 50000 HRS at 25°C

**Input**

Input Voltage: 90~264VAC
Input Current (Max): 0.54A

**Output**Output Voltage: 5V~48V
Output Power (Max): 20W

**General Specification**Ripple Noise: 2%
Efficiency: >=80%
Operating Temperature: 0~40 degree C
Storage Temperature: -20~85 degree C
Over Voltage Protection:Auto Recovery
Short Circuit Protecton: Auto Recovery
Meet CE, FCC
Dimension: 75 \*48\*26mm

