 [www.astekglobe.com](http://www.astekglobe.com)

**APP062 60W Open Frame/Enclosed Switching Power Supply**

**Feature**

\*Over Voltage Protection, Over Current Protection, Short Circuit Protection

\*100% Burn in test at 40°C

\*Low Ripple Noise, MTBF Above 50000 HRS at 25°C

**Input**

Input Voltage: 90~264VAC
Input Current (Max): 2A

**Output**
Output Voltage: 24V~48V
Output Power (Max): 60W
Ripple Noise: 500mA
Efficiency: >=80%

**General Specification**
Operating Temperature: -40~70 degree C
Storage Temperature: -40~90 degree C
Over Voltage Protection:Auto Recovery
Short Circuit Protecton: Auto Recovery
Meet CE, FCC
Dimension: 147.4 \* 84mm

