 [www.astekglobe.com](http://www.astekglobe.com)

**APP075 75W Open Frame/Enclosed Switching Power Supply**

**Feature**

\*Over Voltage Protection, Over Current Protection, Short Circuit Protection

\*100% Burn in test at 40°C

\*Low Ripple Noise

\*MTBF Above 50000 HRS at 25°C

**Input**

Input Voltage: 90~264VAC
Input Current (Max): 1.5A

**Output**
Output Voltage: 5V~48V
Output Power (Max): 75W
Ripple Noise: 1%
Efficiency: >=80%

**General Specification**Operating Temperature: -20~55 degree C
Storage Temperature: -20~85 degree C
Over Voltage Protection:Auto Recovery
Short Circuit Protecton: Auto Recovery
Meet CE, FCC
Dimension: 130 \* 98 \*40mm

