 [www.astekglobe.com](http://www.astekglobe.com)

**APP160 Series**

160W Single Output Voltage Open Frame/Enclosed Power Supply

**Feature**

\*Over Voltage Protection, Over Current Protection, Short Circuit Protection

\*100% Burn in test at 40°C

\*Low Ripple Noise MTBF Above 50000 HRS at 25°C

**Input**

Input Voltage: 90~264VAC
Input Current (Max): 2.5A

**Output**Output Voltage: 5V~48V
Output Power (Max): 150W

**General Specification**
Ripple Noise: 1%
Efficiency: >=89%
Operating Temperature: -20~55 degree C
Storage Temperature: -20~85 degree C
Over Voltage Protection:Auto Recovery
Short Circuit Protecton: Auto Recovery
Meet CE, FCC
Dimension: 159 \* 98.5 \*42.5mm

