 [www.astekglobe.com](http://www.astekglobe.com)

**APP300 Series**

300W Single Output Voltage Open Frame/Enclosed Power Supply

**Feature**

\*Over Voltage Protection, Over Current Protection, Short Circuit Protection

\*100% Burn in test at 40°C

\* Low Ripple Noise

\*MTBF Above 50000 HRS at 25°C

**Input**

Input Voltage: 90~264VAC
Input Current (Max): 7A

**Output**Output Voltage: 12V~48V
Output Power (Max): 300W
Ripple Noise: 1%
Efficiency: >=87%

**General Specification**Operating Temperature: 0~40 degree C
Storage Temperature: -20~70 degree C
Over Voltage Protection:Auto Recovery
Short Circuit Protecton: Auto Recovery
Meet CE, FCC
Dimension: 199 \* 110 \*50mm