 [www.astekglobe.com](http://www.astekglobe.com)

APD010/APD020 SERIES 10-20W DC DC Car Charger

Features

\*DC DC Car Adapter

\*Non-Isolated

\*Protections: Short Circuit/Overcurrent/ Overvoltage

\*Low Ripple Noise

\*100% Burn-in test High Ambient Temp(40°C)

Application: Car charger, Automobile charger, Vehicle adapter

**Input**

Voltage: 10.5-28VDC

Input current: 3A max.

**Output**

Over Voltage Protection/Short Circuit Protection: Auto Recovery

Ripple & Noise: 300mV max.

**Part No O/P Voltage O/P Current(max.) watt Max**

**APD010-S09 3~9V 3A 10W**

**APD020-S09 3-9V 4A 20W**

**General Specification**

Efficiency Level : >=85%

Operating Temperature: 0~40degree C

Storage Temperature: -20~85degree C

Safety: Meet CE and FCC

 Mechanical Drawing

 