C:\Users\alice\Desktop\2016 website\astekglobe logo.bmp [www.astekglobe.com](http://www.astekglobe.com)

APD040 SERIES 40W DC DC Car Charger

Features

\*DC DC Car Adapter

\*Protections: Short Circuit/Overcurrent/ Overvoltage

\*Low Ripple Noise

\*100% Burn-in test High Ambient Temp(40°C)

\*Application: Car charger, Automobile charger, Vehicle adapter

**Input**

Voltage: 10.5-28VDC

Input current: 4A max.

**Output**

Over Voltage Protection/Short Circuit Protection: Auto Recovery

Ripple & Noise: 200mV max.

**Part No O/P Voltage O/P Current(max.) watt Max**

**APD040 12~24V 3.3A 40W**

**General Specification**

Efficiency Level : >=85%

Operating Temperature: 0~40degree C

Storage Temperature: -20~85degree C

Safety: Meet CE and FCC

Mechanical Drawing

